|  |  |  |
| --- | --- | --- |
| № | Word or phrase | Meaning |
| 1 | Active-matrix | a display system in which each pixel is individually controlled |
| 2 | Brightness | the luminance of images |
| 3 | Cartridge | a container holding a quantity of ink, designed for insertion into a ink-jet printer |
| 4 | Cathode Ray Tube (CRT) | a high-vacuum tube in which cathode rays produce a luminous image on a fluorescent screen, used chiefly in televisions and computer terminals |
| 5 | Colour depth | the number of colours a monitor can display |
| 6 | Digital light-processing | device which creates the image with millions of microscopic mirrors arranged on a silicon chip |
| 7 | Display resolution | the number of distinct pixels in each dimension that can be displayed |
| 8 | Dot-matrix printer | a printer that forms images of letters, numbers, etc., from a number of tiny dots. |
| 9 | Dpi(dots per inch) | measure of the output quality |
| 10 | Front-screen projector | an image projector that receives a video signal and projects the corresponding image on a projection screen using a lens system |
| 11 | Home cinema | home entertainment audio-visual systems that seek to reproduce a movie theater experience |
| 12 | Imagesetter | a very high-quality type of color printer used to print glossy magazines, newsletters, or other documents |
| 13 | Impact printing | technology allows to print multi-part forms |
| 14 | Ink-jet printer | a printer in which the characters are formed by minute jets of ink |
| 15 | Laser printer | a printer, producing good-quality printed material by using a laser to form a pattern of electrostatically charged dots on a light-sensitive drum, which attract toner (or dry ink powder) |
| 16 | Liquid Crystal Display (LCD) | a form of visual display used in electronic devices in which a layer of a liquid crystal is sandwiched between two transparent electrodes |
| 17 | Monitor | an instrument or device used for observing, checking, or keeping a continuous record of a process or quantity |
| 18 | Multi-functional printer | a printer which incorporates the functionality of multiple devices in one (a typical MFP may act as a combination of some or all of the following devices: email, fax, photocopier, printer, scanner) |
| 19 | Page description language (PDL) | a computer language that describes the appearance of a printed page in a higher level than an actual output bitmap |
| 20 | Pages per minute(ppm) | measure of the speed of printer |
| 21 | Phosphor | substance in CRT monitor which glow and create colours |
| 22 | Pin | an electronic device for storing and processing data, typically in binary form, according to instructions given to it in a variable program |
| 23 | Plasma display | a type of flat panel display that uses small cells containing plasma; ionized gas that responds to electric fields |
| 24 | Plotter | a computer printer for printing vector graphics |
| 25 | Primary color | any of a group of colors from which all other colors can be obtained by mixing |
| 26 | Print Server | computer that stores the files waiting to be printed, also allows users to share a printer |
| 27 | Print spooler | a program stores files to be printed when the printer is ready |
| 28 | Printer | device that prints your texts or graphics on paper |
| 29 | Printer driver | a piece of software on a computer that converts the data to be printed to a format that a printer can understand |
| 30 | Printer resolution | the printout quality |
| 31 | Printout | the output on paper or acetate sheets |
| 32 | Rear projection TV | a type of large-screen television display technology |
| 33 | Refresh rate | the number of times that the image is drawn each second |
| 34 | Screen size | the physical size of the area where pictures and videos are displayed |